## Main Function:

- ### Dynamic Domain Name Service For DVR Device(88110.net)

- ### Local Device Manage。

- ### Real Time Video Surveillance。

- ### PTZ Control。

- ### Record And Snapshot。

- ### Remote Parameter Configuration ,Account Manager。

## Main Fuction Operational Progress:

## 1.Dynamic Domain Name Service For DVR Device

There are two ways for you to login: normal and the 88110 server .

If your DVR devices are via ADSL Internet or Device’IP is dynamic,you can use our 88110 serve for free.

Within LAN,static ip,and using the third domain service.you can login in by normal.

1.1 Normal Login

### 1.2 88110 server

Start software click the Login Type > Normal .Switch login type.

choose 88110.net

Choose 88110 server login: username and password of 88110 server are the same as which registered in the www.88110.net.

## 2.Device Manager

### 2.1 Adding Device

Click，Enter the interface of device management. Click the right upper corner "+" to add a device.

Click done,return to device list interface. The newly add-up device will be shown in the list.

.

### 2.2 Edit a device

Click upper left "Edit", click the device name, enter the device information edit interface; Click "Delete" to delete the device.

Click upper left "Done" to return to device management interface.

## 3.Real Tme Video Surveillance

After adding the device, live view of channels can be operated.

click，Enter the live view interface(the default interface after login the firmware is the live view interface).

After entering the live view interface, select upper right "Device", click and choose the device, live view the images.

Click the liveview button to view all CHs of the device

Live view window buttons are defined as below:

Button | Definition
| PTZ control button
| Record of all the channels
| Capture images of all the channels
| Stop live view of all the channels
| Audio of all the channels

Enlarge the live view :

1、1. Double click the CH to full screen this CH. Double click again to go back to the 4 CH live view.

2、wipe 2 figures to full screen the CH or go back to 4CH live view.

. A right or left swipe jumps from one CH to the next CH like opening book pages.

## 4.PTZ Control

choose the focus chanel,clickto enable the PTZ. Click the direction button to control the camera.

Swipe to zoom in or zoom out.

## 5.Record Control And Snapshot

### 5.1 Local Record

choose the focus chanel,，clickto enable the local record function. This button will be in red when recording.Click this button again to stop recording

recorde will be auto-save.

### 5.2Local Record Playback

click，and then click entering the playback interface

Playback instruction:

configuration | Explain
RemotePlayback | Playback the recordings in the DVR remotely
Event Playback | Playback the alarms
Local Playback | Playback the recordings in the mobile phone
Picture Playback | View and playback the snapshot picture

Double click the files in the list to start local playback.

Delete Video Files:

Drag the icon > to left to delete the files.

### 5.3RemotePlayback

click ，entering the playback interface,Click “Select” to select the remote device.

Then the list of recordings will be created. Select the date then the list of recording of that date will be created.

### 5.4Picture Playback

click，entering the playback interface,to playback the image

click ”:，save picture ，click “”,delete picture。

### 5.5 Snapshot

choose the living view，click，and then click save or cancel button.

## 6.Remote Parameter Configuration

### 6.1 Remote Configuration

click ，entering parameter configuration interface。

Choose the device first, and then enter the settings like bellow.

you can sitch the Screen orientation by rotating iphone or ipad when full-screen.

### 6.2other configuration

More settings are lists here：System, About. Click，entering the interface.

You can set the network and PTZ speed and others here in local system

PTZ Speed:PTZ speed,More to the right, a camera rotating the larger amplitude.

Network:Is only allowed to work in WiFi network.